Tests for Huber Machine Program

\*\*\* All checks must be run after new release!

1. “Only UP” from -20 ˚C to 136˚C.
   1. Sto (0.08/0.1/0.2/0.3…)
   2. Str (Value in mm on target Temperature)
   3. Str Max (Value in mm on target Temperature)
   4. Time of running program
   5. Check impossibility of entering “low Temperature” higher than “high Temperature.